Nick Moore

Lab 5.8

Table 5.11 Wall Outlet AC Checks

|  |  |  |
| --- | --- | --- |
| **Connections** | **Expected Voltage** | **Actual Voltage** |
| GND to Hot | 120VAC | 119.8 |
| GND to Neutral | 0VAC | .85 |
| Hot to Neutral | 120VAC | 118.0 |

Table 5.12 Power Cord AC Checks

|  |  |  |
| --- | --- | --- |
| **Connections** | **Expected Voltage** | **Actual Voltage** |
| GND to Hot | 120VAC | 119.6 |
| GND to Neutral | 0VAC | .23 |
| Hot to Neutral | 120VAC | 119.1 |